<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<packages>
<package name="18650-PC4">
</package>
<package name="12-MSOP">
</package>
<package name="4HEAD_MOLEX_C71308">
</package>
<package name="SOIC-16">
</package>
<package name="TSSOP-8">
</package>
</packages>
<symbols>
<symbol name="2CELLBATT">
<pin name="-2"/>
<pin name="+1"/>
<pin name="-1"/>
<pin name="+2"/>
</symbol>
<symbol name="LT3650">
<pin name="VIN"/>
<pin name="CLP"/>
<pin name="!SHDN"/>
<pin name="!CHRG"/>
<pin name="!FAULT"/>
<pin name="TIMER"/>
<pin name="RNG/SS"/>
<pin name="NTC"/>
<pin name="BAT"/>
<pin name="SENSE"/>
<pin name="BOOST"/>
<pin name="SW"/>
<pin name="GND"/>
</symbol>
<symbol name="SMT_HEADER_4">
<pin name="1"/>
<pin name="2"/>
<pin name="4"/>
<pin name="3"/>
</symbol>
<symbol name="UCC3911">
<pin name="NC"/>
<pin name="!OV"/>
<pin name="!UV"/>
<pin name="SUBS1"/>
<pin name="SUBS2"/>
<pin name="GND"/>
<pin name="GND2"/>
<pin name="LPWARN"/>
<pin name="B2"/>
<pin name="CDLY"/>
<pin name="B1"/>
<pin name="SUBS4"/>
<pin name="SUBS3"/>
<pin name="B0.2"/>
<pin name="B0.1"/>
<pin name="CE"/>
</symbol>
<symbol name="BQ2057">
<pin name="SNS"/>
<pin name="BAT"/>
<pin name="VCC"/>
<pin name="TS"/>
<pin name="COMP"/>
<pin name="CC"/>
<pin name="VSS"/>
<pin name="STAT"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BK-18650-PC4">
<gates>
<gate name="G$1" symbol="2CELLBATT"/>
</gates>
<devices>
<device name="" package="18650-PC4">
<connects>
<connect gate="G$1" pin="+1" pad="+1"/>
<connect gate="G$1" pin="+2" pad="+2"/>
<connect gate="G$1" pin="-1" pad="-1"/>
<connect gate="G$1" pin="-2" pad="-2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3650">
<description>A monolithic two cell lithium ion charger.</description>
<gates>
<gate name="G$1" symbol="LT3650"/>
</gates>
<devices>
<device name="" package="12-MSOP">
<connects>
<connect gate="G$1" pin="!CHRG" pad="4"/>
<connect gate="G$1" pin="!FAULT" pad="5"/>
<connect gate="G$1" pin="!SHDN" pad="3"/>
<connect gate="G$1" pin="BAT" pad="9"/>
<connect gate="G$1" pin="BOOST" pad="11"/>
<connect gate="G$1" pin="CLP" pad="2"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NTC" pad="8"/>
<connect gate="G$1" pin="RNG/SS" pad="7"/>
<connect gate="G$1" pin="SENSE" pad="10"/>
<connect gate="G$1" pin="SW" pad="12"/>
<connect gate="G$1" pin="TIMER" pad="6"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C-GRID-71308">
<description>4 Pin SMT Molex HEADER
Digikey: WM17450-ND</description>
<gates>
<gate name="G$1" symbol="SMT_HEADER_4"/>
</gates>
<devices>
<device name="" package="4HEAD_MOLEX_C71308">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UCC3911">
<gates>
<gate name="G$1" symbol="UCC3911"/>
</gates>
<devices>
<device name="" package="SOIC-16">
<connects>
<connect gate="G$1" pin="!OV" pad="2"/>
<connect gate="G$1" pin="!UV" pad="3"/>
<connect gate="G$1" pin="B0.1" pad="10"/>
<connect gate="G$1" pin="B0.2" pad="11"/>
<connect gate="G$1" pin="B1" pad="14"/>
<connect gate="G$1" pin="B2" pad="16"/>
<connect gate="G$1" pin="CDLY" pad="15"/>
<connect gate="G$1" pin="CE" pad="9"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$1" pin="LPWARN" pad="8"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="SUBS1" pad="4"/>
<connect gate="G$1" pin="SUBS2" pad="5"/>
<connect gate="G$1" pin="SUBS3" pad="12"/>
<connect gate="G$1" pin="SUBS4" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ2057TTS">
<gates>
<gate name="G$1" symbol="BQ2057"/>
</gates>
<devices>
<device name="" package="TSSOP-8">
<connects>
<connect gate="G$1" pin="BAT" pad="2"/>
<connect gate="G$1" pin="CC" pad="7"/>
<connect gate="G$1" pin="COMP" pad="8"/>
<connect gate="G$1" pin="SNS" pad="1"/>
<connect gate="G$1" pin="STAT" pad="5"/>
<connect gate="G$1" pin="TS" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
