<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="60.96" x2="79.99" y2="60.96" width="0" layer="20"/>
<wire x1="79.99" y1="60.96" x2="80.01" y2="91.11" width="0" layer="20"/>
<wire x1="80.01" y1="91.11" x2="1.27" y2="91.11" width="0" layer="20"/>
<wire x1="1.27" y1="91.11" x2="1.27" y2="60.96" width="0" layer="20"/>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="jabinder">
<packages>
<package name="18650-PC4">
</package>
<package name="4HEAD_MOLEX_C71308">
</package>
<package name="SOIC-16">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="jabinder" package="18650-PC4" value="BK-18650-PC4"/>
<element name="CHRG" library="jabinder" package="4HEAD_MOLEX_C71308" value="C-GRID-71308">
<attribute name="NAME"/>
</element>
<element name="BAT" library="jabinder" package="4HEAD_MOLEX_C71308" value="C-GRID-71308">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="jabinder" package="SOIC-16" value="UCC3911"/>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="330pF">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value="220">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="0.22uF">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0603-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="0.1uF,  25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="jabinder" package="SOIC-16" value="MCP73862"/>
<element name="LED1" library="SparkFun-LED" package="LED-1206" value=""/>
<element name="LED2" library="SparkFun-LED" package="LED-1206" value=""/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="4.7uF"/>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="0.1 uF"/>
<element name="RT1" library="SparkFun-Passives" package="0603-RES" value="14.5k"/>
<element name="RT2" library="SparkFun-Passives" package="0603-RES" value="30.3k"/>
</elements>
<signals>
<signal name="V_BATT+">
<contactref element="U$1" pad="+1"/>
<contactref element="BAT" pad="1"/>
<contactref element="BAT" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="13"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="INTERCELL">
<contactref element="U$1" pad="-1"/>
<contactref element="U$1" pad="+2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="BAT" pad="4"/>
<contactref element="BAT" pad="3"/>
<contactref element="CHRG" pad="4"/>
<contactref element="CHRG" pad="3"/>
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="6"/>
<contactref element="C8" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="11"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="7"/>
<contactref element="RT2" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="CHRG" pad="1"/>
<contactref element="CHRG" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="5"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="N$9">
<contactref element="U2" pad="15"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U2" pad="16"/>
<contactref element="C6" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="V_BATT-">
<contactref element="U$1" pad="-2"/>
<contactref element="U2" pad="10"/>
<contactref element="U2" pad="11"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U2" pad="14"/>
<contactref element="C7" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="9"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="HSINK">
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="13"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="N$4">
<contactref element="LED1" pad="C"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="2"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="1"/>
<contactref element="RT2" pad="2"/>
<contactref element="RT1" pad="1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="8"/>
<contactref element="RT1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
